VTTEST(1) User commands VTTEST(1)

NAME

vttest − test VT100-type terminal SYNOPSIS

vttest [options] [24x80.132] DESCRIPTION Vttest is a program designed to test the functionality of a VT100 terminal (or emulator thereof). It tests both display (escape sequence handling) and keyboard.

The program is menu-driven and contains full on-line operating instructions. • To run a given menu-item, you must enter its number. • Menu items start at zero; this is the “Exit” item in almost all cases. • You can run all menu-items (for a given level) by entering an asterisk, i.e, “*’. • You can force a repaint of the menu items by entering “?”.

• A few menus can be more than one page. Use “n” and “p” to switch to the next or previous page. OPTIONS

You can specify the screen geometry in the form [24x80.132], i.e., • 24 lines, • 80 minimum columns, and • 132 maximum columns.

If your terminal does not switch between 80 and 132 columns you may specify 24x80.80, for example, to avoid a misleading display. Other options are: −V print the program version, and exit. −f fontfile

specify a file containing a DRCS (soft character definition) string. −l log test results to vttest.log. −p use padding, e.g., for a VT100 connected to a high-speed line. −q show only the most recent part of a continuous response, e.g., any-event mouse tests, to improve readability of the test.

−s add time-delay in selected panning/scrolling options to show details. −8 use 8-bit controls (this can be changed with a menu option).

AUTHOR

Per Lindberg (mcvax,seismo)!enea!suadb!lindberg sometime 1985.

Modified by Thomas Dickey from June 1996, to support nonstandard screen geometry, VT220-VT520, ISO color and xterm-specific tests.

2020-09-20 1